L2 trigger

Detector

L3 Farm

MassStorageL1 Accept

Level 2:Asynchronous 2 stage pipeline~20ms latency<1kHz Accept Rate

L1+L2 rejection: 10,000:17.6 MHz Crossing rate132 ns clock cycle

L1 trigger

Level1:7.6 MHz Synchronous pipeline5544ns latency<50 kHz Accept rate

L2 Accept

L1 StoragePipeline:42 Clock Cycles DeepL2 Buffers: 4 EventsDAQ Buffers

PJW 6/2/96Dataflow of CDF "Deadtimeless" Trigger and DAQ