SEtTrigger InformationCS-P3

FromBackplaneOutput to Global Level 1Energy SummaryCrate Sum BoardBack-planeLatch

CS-P1CS-P2

Timing and Control Signals

To DAQDAQ Readout

Manager

8 x SEt16 x Trigger Bits

FoF1CS-FR1TriggerSummary

Board Sum LatchCS-FR1:40 Pin Connector(2 phi Channels x 10 bits sent Differentially)CS-FR2:40 Pin Connector(16 Trigger bits sent Differentially)CS-FR2