DIRAC Card (Level 1)Input cables from detector

1 of 6 Towers shown20

120trackingfan-out

86x396AlignFIFOSRAMThresh+ TrackCardsummary

TO DCAS: 120 bitstower energy for Level 2trigger

TO L1 CRATESUM: 24 bits 2 bit count x 3 trigger types 1 bit count x 10 trigger types 8 bits Sum Et Data (via J3 Backplane)

FROM XTRP: 8 bits trackinfo for thisphi wedge

8+3+89U x 400 mm VME Card

VME Interface

203Data Bufferingfor ReadoutAux Card13 towers In 6+1 HAD 6 EM10 bits/tower130 diff rec.1 10 bit adder 12 towers Out 6 HAD 6 EM 120 bits9U x 120mm

P316SEt848LatchMaskSHAD+EM 120